***FLOW- METER CALIBRATION***

***FLC-Y, SASEBO FUEL DIVISION Date: 05 APR 2023***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Facility / Admin. # | Line # | Description of Flow-Meter | Set Product | Actual Product |
| JP-5 Tank Truck | USN 96-48756  ( J-9 T/T ) | Manufacture : Liquid Control Corporation  Model : M-25-2  Serial No. 473978  Flow Range 30 ~ 300 GPM  Coupling Size : 1-1/2 Cam-lock Coupling | JP-5 | JP-5 |
| F-76 Tank Truck | USN 96-53881 ( F-2 T/T ) | Manufacture : TOKICO Technology LTD  Model : FRP0541BAE-96X2-X  Serial No. 18IFA0128  Flow Range 50 ~ 80 USG/min  Coupling Size : 1-1/2 Cam-lock Coupling | F-76 | F-76 |
| F-76 Tank Truck | USN 96-53460 ( F-3 T/T ) | Manufacture : TOKICO Technology LTD  Model : FRPO541BAE-96X2-X  Serial No. QAA1682  Flow Range 50 ~ 80 USG/ min  Max Operational Pressure : 1.0 mPa  Coupling Size : 1-1/2 Cam-lock Coupling | F-76 | F-76 |
| F-76 Tank Truck | USN 96-53773 ( F-1 T/T ) | Manufacture : TOKICO Technology LTD  Model : FRPO541BAE-96X2-X  Serial No. 17HA0008  Flow Range 50 ~ 80 USG/ min  Max Operational Pressure : 1.0 mPa  Coupling Size : 1-1/2 Cam-lock Coupling | F-76 | F-76 |
| LT-L Tank Truck  (21-90 Turbine Oil ) | USN 96-53882 ( LT-1 T/T ) | Manufacture : TOKICO Technology LTD  Model : FRP0541BAE-96X2-X Serial No. 18IFA0127  Flow Range 50 ~ 80 USG/ min  Max Operational Pressure : 1.0 mPa  Coupling Size : 1-1/2 Cam-lock Coupling | LT-L (21-90 Turbine Oil ) | LT-L (21-90 Turbine Oil ) |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Facility / Admin. # | Line # | Description of Flow-Meter | Set Product | Actual Product |
| F-76 Fuel Barge | YON-290 | Manufacture : Brodie Meter Co., LLC  Model : B90ACAAAACDAAD  Serial No. 1309-29094U-1-2A  Flow Range 100 ~ 1,000 GPM  Coupling Size : 4inch Flange | F-76 | F-76 |
| F-76 Fuel Barge | YON-305 | Manufacture : Liquid Control Corporation  Model : B-090ACAAAACDADD  Serial No. 1309-290940-1-1A  Flow Range 100 ~ 1,000 GPM  Coupling Size : 4inch Flange | F-76 | F-76 |  |